	FENCE INSTALLATION ESTIMATE



	CONTRACTOR
Business name: Example Fence & Gate Co.
Address: 75 Example Lane, Sampletown
Phone / email: [Phone or email]
License no.: [License no., if applicable]
	ESTIMATE DETAILS
Estimate no.: FN-2026-208
Date: 5 Oct 2026
Valid until: 4 Nov 2026
Prepared by: [Estimator name]


CLIENT AND SITE
	Client name
	Lee Sample
	Phone / email
	[Phone or email]

	Site address
	9 Sample Way, Sampletown

	Property line
	From owner's survey (copy on file)

	Utility locate
	811 request before digging; ticket [Ticket no.]


FENCE SPECIFICATION
	Material
	Pressure-treated pine, dog-ear pickets

	Height
	6 ft
	Length
	186 linear ft

	Post spacing
	8 ft on center, 4x4 posts in concrete

	Gates
	1 walk gate, 4 ft wide


OLD FENCE REMOVAL
	Description
	Qty
	Unit
	Unit price
	Amount

	Remove and haul away existing chain-link fence
	160
	lin ft
	3.50
	560.00

	Pull old posts and concrete footings
	21
	ea
	22.00
	462.00

	
	
	
	
	

	Removal subtotal
	1,022.00


MATERIALS
	Description
	Qty
	Unit
	Unit price
	Amount

	Posts, 4x4 x 8 ft treated
	26
	ea
	16.80
	436.80

	Rails, 2x4 x 8 ft treated (3 per section)
	72
	ea
	7.45
	536.40

	Pickets, 1x6 x 6 ft dog-ear
	406
	ea
	3.15
	1,278.90

	Concrete mix, 50 lb bags
	52
	bag
	6.95
	361.40

	Gate hardware kit (hinges, latch, drop rod)
	1
	kit
	68.50
	68.50

	Galvanized nails and screws
	1
	lot
	85.00
	85.00

	
	
	
	
	

	Materials subtotal
	2,767.00


LABOR
	Description
	Qty
	Unit
	Unit price
	Amount

	Dig holes and set posts in concrete
	26
	ea
	38.00
	988.00

	Install rails and pickets
	186
	lin ft
	9.50
	1,767.00

	Build and hang walk gate
	1
	ea
	275.00
	275.00

	
	
	
	
	

	Labor subtotal
	3,030.00



	Subtotal
	6,819.00

	Sales tax, if applicable (0%)
	0.00

	Estimated total
	6,819.00

	Proposed deposit (10%)
	681.90


INCLUDED
1. Removal and disposal of the old fence
1. Materials and labor for the fence and gate specified
1. Clean-up of the work area
NOT INCLUDED
1. Surveying or marking the property line
1. Rock, roots or buried obstructions in post holes (priced before extra work is done)
1. Staining or sealing
BEFORE WORK STARTS
1. Owner confirms the fence line from the survey
1. Underground utilities are marked through the 811 request before any digging
1. Contractor confirms whether a permit is needed; owner confirms any HOA approval

	
	
	

	Accepted by (client signature)
	
	Print name

	
	
	

	Date
	
	Contractor signature


Linear footage measured on site on 3 Oct 2026. Prices are valid until the date shown above.
