	CONCRETE ESTIMATE



	CONCRETE CONTRACTOR
Business name: Example Concrete Co.
Address: 7 Example Yard Road, Sampletown
Phone / email: [Phone or email]
License no.: [License no., if required where you work]
	ESTIMATE DETAILS
Estimate no.: CN-1185
Date: Nov 5, 2026
Valid until: Dec 5, 2026
Prepared by: [Estimator name]


CLIENT AND JOB SITE
	Client name
	Alex Example
	Phone / email
	[Phone or email]

	Job address
	92 Sample Avenue, Sampletown

	Existing surface
	Cracked asphalt driveway, about 4 in. thick


SLAB DETAILS
	Slab type
	Driveway
	Area
	640 sq ft (16 ft by 40 ft)

	Thickness
	4 in.

	Concrete volume
	7.9 cu yd, plus about 7% for waste and grade = 8.5 cu yd

	Finish
	Broom finish, control joints about every 10 ft


REMOVAL AND BASE
	Description
	Qty
	Unit
	Unit price
	Amount

	Break out the old asphalt driveway and load for hauling
	640
	sq ft
	2.25
	1,440.00

	Compacted gravel base, 4 in.
	640
	sq ft
	1.60
	1,024.00

	
	
	
	
	

	Removal and base subtotal
	2,464.00


FORMING AND REINFORCEMENT
	Description
	Qty
	Unit
	Unit price
	Amount

	Forms along the edges
	112
	lin ft
	4.50
	504.00

	Rebar, #4 at 18 in. on center, on chairs
	640
	sq ft
	1.35
	864.00

	Expansion joint at the garage slab
	16
	lin ft
	3.00
	48.00

	
	
	
	
	

	Forming and reinforcement subtotal
	1,416.00


CONCRETE AND FINISHING
	Description
	Qty
	Unit
	Unit price
	Amount

	Ready-mix concrete, 4,000 psi
	8.5
	cu yd
	165.00
	1,402.50

	Place and finish, broom finish
	640
	sq ft
	2.40
	1,536.00

	Saw-cut control joints
	128
	lin ft
	1.25
	160.00

	Cure and seal
	640
	sq ft
	0.45
	288.00

	
	
	
	
	

	Concrete and finishing subtotal
	3,386.50



	Subtotal
	7,266.50

	Disposal fee, passed through
	380.00

	Sales tax on work and materials, if applicable (0%)
	0.00

	Estimated total
	7,646.50


SCOPE NOTES
1. Concrete volume: 640 sq ft at 4 in. thick is 7.9 cu yd; 8.5 cu yd is ordered to allow for waste and grade
1. The disposal fee is the charge for hauling and dumping the old asphalt, passed through at cost
1. Vehicles stay off the new driveway for 7 days after the pour
EXCLUSIONS
1. Permit fees, if any
1. Colored, stamped or exposed-aggregate finishes
1. Removing tree roots larger than 2 in.
1. Repairing landscaping or sprinkler lines disturbed at the edges

	
	
	

	Accepted by (client signature)
	
	Print name

	
	
	

	Date
	
	


Prices are based on the area and thickness shown above and are valid until the date shown.
